Refer to the manufacturer’s owner manual for specific reference

The checklist is to be completed in 2 stages; before the ATV is started and once the ATV is running.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **ATV not started** | | | | | |
| ⭘ Maintenance Records for any documented issues | | | | | |
| **Visual Inspection** | | | | | |
| ⭘ | Leaks – oil, fuel, etc. | ⭘ | Damaged / loose parts | ⭘ | Drive chain – no slack |
| ⭘ | Suspension – no damage or leaks | ⭘ | Axle boots – no tears or leaks | ⭘ | Footboards / Footpegs – clean and free of dirt |
| ⭘ | Debris in the undercarriage | ⭘ | Tire Repair Kit | ⭘ | Fire Extinguisher (secured) |
| ⭘ | First Aid Kit |  |  |  |  |
|  | | | | | |
| **Fluid levels** | | | | | |
| ⭘ | Fuel – full | ⭘ | Oil – clean, full | ⭘ | Coolant – topped-up |
|  | | | | | |
| **Tires / Rims** | | | | | |
| ⭘ | Pressure – correct inflation is 2-6 psi; use a small scale gauge | ⭘ | Tears / Cuts / Wear | ⭘ | Wheel bolts / lug nuts – tight; do not have play |
|  | | | | | |
| **ATV started** | | | | | |
| **Controls** | | | | | |
| ⭘ | Throttle – moves smoothly; snaps back to idle position; throttle limited adjusted to rider | ⭘ | Breaks (hand and foot) – do not pull to one side; within operator’s reach | ⭘ | Steering / handlebars – moves freely without affecting throttle |
| ⭘ | Lights – working | ⭘ | Transmission – engages / shifts smoothly | ⭘ | Ignition Switch – responds to start and turn off engine |

|  |  |  |  |
| --- | --- | --- | --- |
| ATV Unit Reference: |  | Date: |  |
| Operator Signature: |  | Date: |  |
| Supervisor Signature: |  | Date: |  |